**Changing the Mazda tire:**

* Put the wheel lock on and turn it to left with wrench
* **Loosen** (but do not completely remove) the remaining lug nuts in a star-shaped pattern
* Place the jack in one of the designated spots on the undercarriage of the car. Raise it as far as you can go.
  + You’ll have to torque it using the combo of tools found in the spare tire trunk.
* Completely remove the lug nuts along with the tire
* Place on the spare tire now. Start with the wheel lock and then re-fasten other nuts in a star-shaped pattern.
  + You can use your fingers to fasten at first, then finish with the wrench. Tighten as much as possible by putting your body weight on the wrench.
* You’re good to go!